**Lime Microsystems Limited**

Surrey Technology Centre

Occam Road

The Surrey Research Park

Guildford, Surrey GU2 7YG

United Kingdom

Tel: +44 (0) 1483 685 063

e-mail: [enquiries@limemicro.com](mailto:enquiries@limemicro.com)

**LimeSDR-USB**

***- FPGA Gateware Description****-*

REVISION HISTORY

The following table shows the revision history of this document:

|  |  |  |
| --- | --- | --- |
| **Date** | **Version** | **Description of Revisions** |
| 12/07/2018 | 1.0 | Initial version |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Table of Contents**

[REVISION HISTORY 2](#_Toc519154990)

[1 Introduction 4](#_Toc519154991)

[2 FPGA gateware features 5](#_Toc519154992)

[3 Gateware description 6](#_Toc519154993)

[3.1 Main block diagram 6](#_Toc519154994)

[3.2 Clock network 7](#_Toc519154995)

[3.3 Softcore processor – nios\_cpu 8](#_Toc519154996)

[3.3.1 Registers of fpgacfg module 11](#_Toc519154997)

[3.3.2 Registers of pllcfg module 15](#_Toc519154998)

[3.3.3 Registers of tstcfg module 17](#_Toc519154999)

[3.3.4 Registers of periphcfg module 19](#_Toc519155000)

[3.4 FX3 Slave FIFO interface – FX3\_slaveFIFO5b 21](#_Toc519155001)

[3.5 LMS7002 Receive and transmit interface – rxtx\_top 23](#_Toc519155002)

[3.5.1 Receive interface – rx\_path\_top 27](#_Toc519155003)

[3.5.2 Transmit interface – tx\_path\_top 28](#_Toc519155004)

[3.5.3 Waveform player – wfm\_player\_top 30](#_Toc519155005)

[3.6 General periphery – general\_periph\_top 30](#_Toc519155006)

[3.7 PLL module – pll\_top 33](#_Toc519155007)

[3.8 Board test module – tst\_top 37](#_Toc519155008)

[4 Examples 39](#_Toc519155009)

[4.1 Accessing FPGA registers 39](#_Toc519155010)

[4.2 Accessing LMS7002M registers 40](#_Toc519155011)

[4.3 Periphery control 40](#_Toc519155012)

[4.4 Configuring FPGA PLL module 41](#_Toc519155013)

[4.4.1 RX PLL module - rxpll\_top configuration (auto phase shift mode) 41](#_Toc519155014)

[4.4.2 TX PLL module - txpll\_top configuration (auto phase shift mode) 42](#_Toc519155015)

[4.5 Controlling TX and RX data stream 43](#_Toc519155016)

[4.6 Using WFM player 44](#_Toc519155017)

# Introduction

This document contains functional description of FPGA gateware project suited for LimeSDR-USB board.

**FPGA project** - LimeSDR-USB\_lms7\_trx project can be downloaded from GitHub repository

<(https://github.com/myriadrf/LimeSDR-USB_GW)>.

**Required hardware** – LimeSDR-USB v1.4 board.

**Development software** – project is created with Altera Quartus prime, Version 15.1.2 Build 193 02/01/2016 SJ Lite Edition with Cyclone IV device support. Mentioned software edition is free and can be downloaded from [(https://www.altera.com)](https://www.altera.com). Although other Altera Quartus prime software versions supporting Cyclone IV family might work as well but it is recommended to use same version as project was created.

# FPGA gateware features

Gateware contains following features:

* Interface to LMS7002 LimeLightTM digital IQ interface in TRXIQ double data rate mode;
* Real time data transfer between PC and LMS7002 chip.
* Connection to FX3 Slave FIFO interface for transferring data through USB3.0.
* TX samples synchronization with RX samples time stamp;
* SPI connection between LMS7002 chip and other on-board devices;
* WFM player which enables to load waveform to external DDR2 memory from USB3.0 host and translate to LMS7002 RXIQ interface.
* Reconfigurable PLL blocks for LMS7002 clocking.
* Internal SPI registers for FPGA control.

# Gateware description

This chapter describes main modules of LimeSDR-USB\_lms7\_trx project.

## Main block diagram

Cyclone IV FPGAprovides GPIF II interface with FX3 USB3.0 controller. There are two endpoints (EP0F and EP8F) implemented for control data and two endpoints for stream data (EP01 and EP81). Control endpoints are connected to NIOS II softcore processor which provides SPI and I2C communication interfaces for LMS7002M chip, TCXO DAC, ADF4002 phase detector, LM75 temperature sensor. NIOS also provides access to internal SPI configuration registers. Stream endpoints are dedicated for receiving and sending IQ data from/to LMS7002M. **Figure 1** contains top block diagram with main modules. Description of main FPGA instances can be found in **Table 1**.



Figure 1 Top block diagram

Table 1 Description of main instances

| **Instance** | **Description** |
| --- | --- |
| nios\_cpu | NIOS II softcore processor with memory registers. Provides periphery control. See **3.3 Softcore processor – nios\_cpu.** |
| FX3\_slaveFIFO5b\_top | Provides data transfer between external FX3 SuperSpeed USB 3.0 peripheral controller and FPGA. See **3.4 FX3 Slave FIFO interface – FX3\_slaveFIFO5b.** |
| rxtx\_top | Receive and transmit logic between FPGA and external LMS7002 transceiver. See **3.5 LMS7002 Receive and transmit interface – rxtx\_top.** |
| general\_periph\_top | Control module for onboard periphery such as LEDs, GPIO, FAN. See **3.6 General periphery – general\_periph\_top.** |
| pll\_top | Module provides required clocks for rxtx\_top module. See **3.7 PLL module – pll\_top** |
| tst\_top | Board test logic to test external DDR2 memory and external clocks. See **3.8 Board test module – tst\_top.** |

## Clock network

**Figure 2** shows dataflow between main modules and clocking scheme. More details can be found in **Table 2**.



Figure 2 Gateware clock network

Table 2 Clock network description

| **Clock name** | **Frequency, MHz** |  | **Description** |
| --- | --- | --- | --- |
| LMS\_MCLK1 | Configurable | | Sample clock from LMS7002M IC. Used as a reference clock for TXPLL. |
| LMS\_MCLK2 | Configurable | | Sample clock from LMS7002M IC. Used as a reference clock for RXPLL. |
| LMS\_FCLK1 | Configurable | | Sample clock, LMS7002M IC latches LMS\_DIQ1 bus signals using this clock. |
| LMS\_FCLK2 | Configurable | | Not used |
| txpll\_c1 | Configurable | | FPGA launches LMS\_DIQ1 bus signals using this clock. Used for clocking FPGA TX modules. |
| rxpll\_c1 | Configurable | | FPGA latches LMS\_DIQ2 bus signals using this clock. Used for clocking FPGA RX modules. |
| LMK\_CLK | 30.72 | | Reference clock from LMK00105 clock buffer. |
| FX3\_PCLK | 100 | | FX3 USB3.0 GPIF II interface clock. |
| SI\_CLK0 | 27 | | Used for DDR2\_1 memory controller as a reference clock for controller PLL. |
| SI\_CLK1 | 27 | | Used for DDR2\_2 memory controller as a reference clock for controller PLL. |
| SI\_CLK2 | 27 | | Connected only to tst\_top module |
| SI\_CLK3 | 27 | |
| SI\_CLK5 | 27 | |
| SI\_CLK6 | 27 | |
| SI\_CLK7 | 27 | |

## Softcore processor – nios\_cpu

**Figure 3** shows block diagram of nios\_cpu module. This module contains softcore ALTERA NIOS II CPU and user accessible configuration registers for other modules. More detailed description can be found in **Table 3**. Module generic parameters are explained in **Table 4** and ports are described in **Table 5**.



Figure 3 nios\_cpu block diagram

Table 3 Description of nios\_cpu instances

| **Instance** | **Description** |
| --- | --- |
| lms\_ctr | NIOS II softcore processor instance. Processor constantly monitors input FIFO buffer connected to *exfifo\_if* ports and reads one packet containing 64 bytes. See **LMS64C control protocol** document for protocol description and command list. NIOS CPU executes received command and writes 64 bytes response packet to FIFO buffer connected to *exfifo\_of* ports. |
| cfg\_top | Wrapper module for SPI configuration registers. |
| fpgacfg | General configuration 32x16b addressable registers. Address range 0x0000 - 0x001F. See **Table 6** for register description. |
| pllcfg | PLL configuration registers. Address range 0x0020 - 0x003F. See **Table 7** for register description. |
| tstcfg | Test module configuration registers. Address range 0x0060 - 0x007F. see **Table 8** for register description. |
| periphcfg | Peripheral configuration registers. Address range 0x0020 - 0x003F. See **Table 9** for register description. |

Table 4 nios\_cpu module parameters

| **Parameter** | **Type** | **Default** | **Description** |
| --- | --- | --- | --- |
| Start address of SPI registers | | | |
| FPGACFG\_START\_ADDR | integer | 0 | Start address of SPI register modules. Has to be multiple of 32 |
| PLLCFG\_START\_ADDR | integer | 32 |
| TSTCFG\_START\_ADDR | integer | 64 |
| PERIPHCFG\_START\_ADDR | integer | 192 |

Table 5 nios\_cpu module ports

| **Port** | **Type** | **Width** | **Description** |
| --- | --- | --- | --- |
| clk | in | 1 | Free running clock. 100MHz |
| reset\_n | in | 1 | Asynchronous, active low reset |
| Control data FIFO | | | |
| exfifo\_if\_d | in | 32 | External control input FIFO data |
| exfifo\_if\_rd | out | 1 | External control input FIFO read request |
| exfifo\_if\_rdempty | in | 1 | External control input FIFO read empty |
| exfifo\_of\_d | out | 32 | External control output FIFO data |
| exfifo\_of\_wr | out | 1 | External control output FIFO write request |
| exfifo\_of\_wrfull | in | 1 | External control output FIFO write full |
| exfifo\_of\_rst | out | 1 | External control output FIFO reset request, active high |
| SPI 0 | | | |
| spi\_0\_MISO | in | 1 | SPI 0 master input |
| spi\_0\_MOSI | out | 1 | SPI 0 master output |
| spi\_0\_SCLK | out | 1 | SPI 0 clock |
| spi\_0\_SS\_n | out | 5 | SPI 0 slave select. spi\_0\_SS\_n[0] - connected to LMS7002, spi\_0\_SS\_n[1] - to internal SPI modules |
| SPI 1 | | | |
| spi\_1\_MOSI | out | 1 | SPI 1 master output |
| spi\_1\_SCLK | out | 1 | SPI 1 clock |
| spi\_1\_SS\_n | out | 2 | SPI 1 slave select. spi\_1\_SS\_n[0] - connected to onboard TCXO DAC, spi\_1\_SS\_n[1] - to phase detector ADF4002 |
| I2C | | | |
| i2c\_scl | inout | 1 | I2C bus clock, connected to temperature sensor and EEPROM memory. |
| i2c\_sda | inout | 1 | I2C bus data, connected to temperature sensor and EEPROM memory. |
| General purpose I/O | | | |
| gpi | in | 8 | Not used |
| gpo | out | 8 | gpo[0] - indicates NIOS activity. 0 - Idle, 1 - Busy.  gpo[7-1] - not used |
| LMS7002 control | | | |
| lms\_ctr\_gpio | out | 4 | lms\_ctr\_gpio[0] - LMS7002 reset. lms\_ctr\_gpio[3-1] - not used |
| Configuration registers | | | |
| from\_fpgacfg | out | 512 | Input/output ports from/to SPI configuration registers |
| to\_fpgacfg | in | 512 |
| from\_pllcfg | out | 512 |
| to\_pllcfg | in | 512 |
| from\_tstcfg | out | 512 |
| to\_tstcfg | in | 512 |
| to\_tstcfg\_from\_rxtx | in | 512 |
| to\_periphcfg | in | 512 |
| from\_periphcfg | out | 512 |

### Registers of fpgacfg module

Table 6 Register description of fpgacfg module

| **Address** | **Def. value** | **Bits** | **Name** | **Description** |
| --- | --- | --- | --- | --- |
| 0x0000 |  |  | **Board identification number** | |
| 15-0 | **Board ID** | LimeSDR-USB (**Default 000E**) |
| 0x0001 |  | **Gateware version control** | | |
| 15-0 | **GW\_VER** | Gatewate version number |
| 0x0002 |  | **Gateware revision control** | | |
| 15-0 | **GW\_REV** | Gateware revision number |
| 0x0003 |  | **Board version control** | | |
| 15-7 | Reserved |  |
| 6-4 | **BOM\_VER** | Bill of material version |
| 3-0 | **HW\_VER** | Hardware version. |
| 0x0004 | 0000 | 15-0 | Reserved |  |
| 0x0005 | 0000 | **Clock source selection for TX and RX interfaces** | | |
| 15-2 | Reserved |  |
| 1 | **DRCT\_CLK\_EN** | RX clk: |
| 0 - PLL source **(Default)** |
| 1 - Direct clock source |
| 0 | TX clk: |
| 0 - PLL source **(Default)** |
| 1 - Direct clock source |
| 0x0006 | 0000 | 15-0 | Reserved |  |
| 0x0007 | 0303 | **RX TX MIMO Channel control** | | |
| 15-10 | Reserved |  |
| 9 | **CH\_EN** | TX ch. 1: |
| 0 - Disabled |
| 1 - Enabled **(Default)** |
| 8 | TX ch. 0: |
| 0 - Disabled |
| 1 - Enabled **(Default)** |
| 7-2 | Reserved |  |
| 1 | **CH\_EN** | RX ch. 1: |
| 0 - Disabled |
| 1 - Enabled **(Default)** |
| 0 | RX ch. 0: |
| 0 - Disabled |
| 1 - Enabled **(Default)** |
| 0x0008 | 0102 | **DIQ interface control** | | |
| 15-11 | Reserved |  |
| 10 | **DLB\_EN** | Not used |
| 9 | **SYNCH\_DIS** | Packets synchronization using timestamps: |
| 0 - Enabled |
| 1 - Disabled **(Default)** |
| 8 | **MIMO\_INT\_EN** | MIMO mode: |
| 0 - Disabled |
| 1 - Enabled **(Default)** |
| 7 | **TRIQ\_PULSE** | TRXIQ\_pulse mode: |
| 0 - OFF **(Default)** |
| 1 - ON |
| 6 | **DDR\_EN** | DIQ interface mode: |
| 0 - SDR |
| 1 - DDR **(Default)** |
| 5 | **MODE** | Limelight port mode: |
| 0 - TRXIQ **(Default)** |
| 1 - JESD207 (Currently not implemented) |
| 4-2 | Reserved |  |
| 1-0 | **SMPL\_WIDTH** | Interface sample width selection: |
| "10" - 12bit **(Default)** |
| "01" - Do not use |
| "00" - 16bit |
| 0x0009 | 0003 | **Packet control** | | |
| 15-2 | Reserved |  |
| 1 | **TXPCT\_LOSS\_CLR** | TX packets dropping flag clear: |
| 0 - Normal operation **(Default)** |
| 1 - Rising edge clears flag |
| 0 | **SMPL\_NR\_CLR** | Reset timestamp: |
| 0 - Normal operation **(Default)** |
| 1 - Timestamp is cleared |
| 0x000A | 0000 | **RX and TX module control** | | |
| 15-10 | Reserved |  |
| 9 | **TX\_PTRN\_EN** | Test pattern on TX: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 8 | **RX\_PTRN\_EN** | Test pattern on RX: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 7-2 | Reserved |  |
| 1 | **TX\_EN** | TX chain: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 0 | **RX\_EN** | RX chain: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 0x000B | 0000 | 15-0 | Reserved |  |
| 0x000C | 0003 | **WFM player control 1** | | |
| 15-2 | Reserved |  |
| 1 | **WFM\_CH\_EN** | WFM ch.1: |
| 0 - Disabled |
| 1 - Enabled **(Default)** |
| 0 | WFM ch.0: |
| 0 - Disabled |
| 1 - Enabled **(Default)** |
| 0x000D | 0001 | **WFM player control 2** | | |
| 15-3 | Reserved |  |
| 2 | **WFM\_LOAD** | WFM player file load: |
| 0 to 1 transition starts WFM file loading |
| 0 - WFM file loading disabled **(Default)** |
| 1 | **WFM\_PLAY** | WFM player loaded file play enable: |
| 0 - Disabled |
| 1 - Enabled **(Default)** |
| 0 | Reserved |  |
| 0x000E | 0002 | **WFM player control 3** | | |
| 15-2 | Reserved |  |
| 1-0 | **WFM\_SMPL\_WIDTH** | WFM player sample width control: |
| "10" - 12bit, **(Default)** |
| "01" - Do not use |
| "00" - 16bit |
| 0x000F | 0000 | 15-0 | Reserved |  |
| 0x0010 | 0000 | 15-0 | Reserved |  |
| 0x0011 | 0000 | 15-0 | Reserved |  |
| 0x0012 | FFFF | **Controlled SPI enable** | | |
| 15-8 | Reserved | Not used |
| 7 | **SPI\_SS7** |
| 6 | **SPI\_SS6** |
| 5 | **SPI\_SS5** |
| 4 | **SPI\_SS4** |
| 3 | **SPI\_SS3** |
| 2 | **SPI\_SS2** |
| 1 | **SPI\_SS1** |
| 0 | **SPI\_SS0** |
| 0x0013 | 6F6F | **LMS7002 MISC pin control** | | |
| 15 | Reserved |  |
| 14 | **LMS2\_RXEN** | Not used |
| 13 | **LMS2\_TXEN** |
| 12 | **LMS2\_TXNRX2** |
| 11 | **LMS2\_TXNRX1** |
| 10 | **LMS2\_CORE\_LDO\_EN** |
| 9 | **LMS2\_RESET** |
| 8 | **LMS2\_SS** |
| 7 | Reserved |  |
| 6 | **LMS1\_RXEN** | RX hard enable: |
| 0 - Disabled |
| 1 - Enabled **(Default)** |
| 5 | **LMS1\_TXEN** | TX hard enable: |
| 0 - Disabled |
| 1 - Enabled **(Default)** |
| 4 | **LMS1\_TXNRX2** | Port 2 mode selection: |
| 0 - TXIQ **(Default)** |
| 1 - RXIQ |
| 3 | **LMS1\_TXNRX1** | Port 1 mode selection: |
| 0 - TXIQ |
| 1 - RXIQ (**Default)** |
| 2 | **LMS1\_CORE\_LDO\_EN** | Internal LDO control: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 1 | **LMS1\_RESET** | Hardware reset: |
| 0 - Reset activated |
| 1 - Reset inactive **(Default)** |
| 0 | **LMS1\_SS** | Not used |
| 0x0014 | 0000 | 15-0 | Reserved for lms3\_4 |  |
| 0x0015 | 0000 | 15-0 | Reserved for lms5-6 |  |
| 0x0016 | 0000 | 15-0 | Reserved for lms7-8 |  |
| 0x0017 | 0000 | **GPIO for external periphery** | | |
| 15-14 | Reserved |  |
| 13 | **GPIO13** | Not used |
| 12 | **GPIO12** |
| 11 | **GPIO11** |
| 10 | **GPIO10** |
| 9 | **GPIO9** |
| 8 | **GPIO8** |
| 7 | **GPIO7** |
| 6 | **GPIO6** | Ch. B shunt: |
| 0 - Disabled |
| 1 - Enabled **(Default)** |
| 5 | **GPIO5** | Ch. B attenuator |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 4 | **GPIO4** | RF loopback ch. B: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 3 | **GPIO3** | Reserved |
| 2 | **GPIO2** | Ch. A shunt: |
| 0 - Disabled |
| 1 - Enabled **(Default)** |
| 1 | **GPIO1** | Ch. A attenuator: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 0 | **GPIO0** | RF loopback ch. A: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 0x0018 | 0001 | 15-1 | Reserved |  |
| 0 | **DEV\_CTRL0** | Not used |
| 0x0019 |  | 15-0 | Reserved |  |
| 0x001A | 0000 | **Onboard led control** | | |
| 15 | Reserved |  |
| 14 | Reserved |
| 13 | Reserved |
| 12 | Reserved |
| 11 | Reserved |
| 10 | Reserved |
| 9 | Reserved |
| 8 | Reserved |
| 7 | Reserved |
| 6 | **FPGA\_LED2\_G** | Green LED2 control, do not turn on while red LED2 is on: |
| 0 - OFF **(Default)** |
| 1 - ON |
| 5 | **FPGA\_LED2\_R** | Red LED2 control, do not turn on while green LED2 is on: |
| 0 - OFF **(Default)** |
| 1 - ON |
| 4 | **FPGA\_LED2\_OVRD** | LED2 control override: |
| 0 - OFF **(Default)** |
| 1 - ON |
| 3 | Reserved |  |
| 2 | **FPGA\_LED1\_G** | Green LED1 control, do not turn on while red LED1 is on: |
| 0 - OFF **(Default)** |
| 1 - ON |
| 1 | **FPGA\_LED1\_R** | Red LED1 control, do not turn on while green LED1 is on: |
| 0 - OFF **(Default)** |
| 1 - ON |
| 0 | **FPGA\_LED1\_OVRD** | LED1 control override: |
| 0 - OFF **(Default)** |
| 1 - ON |
| 0x001B | 0000 | 15-8 | Reserved |  |
| 7 | Reserved |
| 6 | Reserved |
| 5 | Reserved |
| 4 | Reserved |
| 3 | Reserved |
| 2 | Reserved |
| 1 | Reserved |
| 0 | Reserved |
| 0x001C | 0000 | 15-3 | Reserved | Onboard led control |
| 2 | **FX3\_LED\_G** | Green FX3 control, do not turn on while red FX3 is on: |
| 0 - OFF **(Default)** |
| 1 - ON |
| 1 | **FX3\_LED\_R** | Red FX3 control, do not turn on while green FX3 is on: |
| 0 - OFF **(Default)** |
| 1 - ON |
| 0 | **FX3\_LED\_OVRD** | FX3 control override: |
| 0 - OFF **(Default)** |
| 1 - ON |
| 0x001D | 0000 | 15-0 | Reserved |  |
| 0x001E | 0000 | 15-0 | Reserved |  |
| 0x001F | 0000 | 15-0 | Reserved |  |

### Registers of pllcfg module

Table 7 Register description of pllcfg module

| **Address** | **Def. value** | **Bits** | **Name** | **Description** |
| --- | --- | --- | --- | --- |
| 0x0020 | 0000 | 15-0 | Reserved |  |
| 0x0021 | 0001 |  | **PLL configuration status** | |
| 15-4 | Reserved |  |
| 3 | **AUTO\_PHCFG\_ERR** | Auto phase configuration error status: |
| 0 – no error |
| 1 – Error |
| 2 | **AUTO\_PHCFG\_DONE** | Auto phase configuration status: |
| 0 – Not done |
| 1 – Done |
| 1 | **BUSY** | PLL reconfiguration busy status: |
| 0 – Idle |
| 1 – Busy |
| 0 | **DONE** | PLL configuration status: |
| 0 – Not done |
| 1 – Done |
| 0x0022 | 0000 |  | **PLL lock status** | |
| 15-2 | Reserved |  |
| 1 | **PLL\_LOCK** | RX PLL: |
| 0 – No lock |
| 1 – Locked |
| 0 | TX PLL: |
| 0 – No lock |
| 1 – Locked |
| 0x0023 | 0000 |  | **PLL control** | |
| 15 | Reserved |  |
| 14 | **PHCFG\_MODE** | PLL phase configuration mode: |
| 0 - Manual |
| 1 - AUTO |
| 13 | **PHCFG\_UpDn** | Phase shift direction: |
| 0 - Down |
| 1 - Up |
| 12-8 | **CNT\_IND** | Counter index for phase shift: |
| 0000 - All output counters |
| 0001 - M counter |
| 0010 - C0 counter |
| 0011 - C1 counter |
| 7-3 | **PLL\_IND** | PLL index for reconfiguration: |
| 0000 - TX PLL |
| 0001 - RX PLL |
| Do not use other index values |
| 2 | **PLLRST\_START** | Reset bit for PLL: |
| 0 - Reset inactive |
| 0 to 1 transition triggers reset for PLL with selected index |
| 1 | **PHCFG\_START** | Phase shift start: |
| 0 - Phase shift process inactive |
| 0 to 1 - transition triggers phase shift process for PLL with selected indexes |
| 0 | **PLLCFG\_START** | PLL reconfiguration start: |
| 0 - Phase shift process inactive |
| 0 to 1 - transition triggers phase shift process for PLL with selected indexes |
| 0x0024 | 0000 |  | **PLL reconfiguration settings** | |
| 15-0 | **CNT\_PHASE** | Counter phase value |
| 0x0025 | 01F0 | 15 | Reserved |  |
| 14-11 | **PLLCFG\_BS** | Bandwidth setting (Not used) |
| 10-8 | **CHP\_CURR** | PLL charge Pump Current (1) |
| 7 | **PLLCFG\_VCODIV** | PLL VCO division value |
| 0 = 2 |
| 1 = 1 |
| 6-2 | **PLLCFG\_LF\_RES** | PLL Loop filter resistance (1) |
| 1-0 | **PLLCFG\_LF\_CAP** | PLL Loop filter capacitance (1) |
| 0x0026 | 0001 | 15-4 | Reserved | Counter bypass and odd division control bits (1) |
| 3 | **M\_ODDDIV** |
| 2 | **M\_BYP** |
| 1 | **N\_ODDDIV** |
| 0 | **N\_BYP** |
| 0x0027 | 555A | 15 | **C7\_ODDDIV** |
| 14 | **C7\_BYP** |
| 13 | **C6\_ODDDIV** |
| 12 | **C6\_BYP** |
| 11 | **C5\_ODDDIV** |
| 10 | **C5\_BYP** |
| 9 | **C4\_ODDDIV** |
| 8 | **C4\_BYP** |
| 7 | **C3\_ODDDIV** |
| 6 | **C3\_BYP** |
| 5 | **C2\_ODDDIV** |
| 4 | **C2\_BYP** |
| 3 | **C1\_ODDDIV** |
| 2 | **C1\_BYP** |
| 1 | **C0\_ODDDIV** |
| 0 | **C0\_BYP** |
| 0x0028 | 5555 | 15 | **C15\_ODDDIV** |
| 14 | **C15\_BYP** |
| 13 | **C14\_ODDDIV** |
| 12 | **C14\_BYP** |
| 11 | **C13\_ODDDIV** |
| 10 | **C13\_BYP** |
| 9 | **C12\_ODDDIV** |
| 8 | **C12\_BYP** |
| 7 | **C11\_ODDDIV** |
| 6 | **C11\_BYP** |
| 5 | **C10\_ODDDIV** |
| 4 | **C10\_BYP** |
| 3 | **C9\_ODDDIV** |
| 2 | **C9\_BYP** |
| 1 | **C8\_ODDDIV** |
| 0 | **C8\_BYP** |
| 0x0029 |  | 15-0 | Reserved |  |
| 0x002A | 0000 | 15-8 | **N\_HCNT[15:8]** | N counter values (1) |
| 7-0 | **N\_LCNT[7:0]** |
| 0x002B | 0000 | 15-8 | **M\_HCNT[15:8]** | M counter values (1) |
| 7-0 | **M\_LCNT[7:0]** |
| 0x002C | 0000 | 15-0 | **M\_FRAC[15:0]** | M fractional counter values (Only for fractional PLL) (1) |
| 0x002D | 0000 | 15-0 | **M\_FRAC[31:16]** |
| 0x002E | 0000 | 15-8 | **C0\_HCNT[15:8]** | C0 counter values (1) |
| 7-0 | **C0\_LCNT[7:0]** |
| 0x002F | 0000 | 15-8 | **C1\_HCNT[15:8]** | C1 counter values (1) |
| 7-0 | **C1\_LCNT[7:0]** |
| 0x0030 | 0000 | 15-8 | **C2\_HCNT[15:8]** | C2counter values (1) |
| 7-0 | **C2\_LCNT[7:0]** |
| 0x0031 | 0000 | 15-8 | **C3\_HCNT[15:8]** | C3 counter values (1) |
| 7-0 | **C3\_LCNT[7:0]** |
| 0x0032 | 0000 | 15-8 | **C4\_HCNT[15:8]** | C4 counter values (1) |
| 7-0 | **C4\_LCNT[7:0]** |
| 0x0033 | 0000 | 15-8 | **C5\_HCNT[15:8]** | C5 counter values (1) |
| 7-0 | **C5\_LCNT[7:0]** |
| 0x0034 | 0000 | 15-8 | **C6\_HCNT[15:8]** | C6 counter values (1) |
| 7-0 | **C6\_LCNT[7:0]** |
| 0x0035 | 0000 | 15-8 | **C7\_HCNT[15:8]** | C7 counter values (1) |
| 7-0 | **C7\_LCNT[7:0]** |
| 0x0036 | 0000 | 15-8 | **C8\_HCNT[15:8]** | C8 counter values (1) |
| 7-0 | **C8\_LCNT[7:0]** |
| 0x0037 | 0000 | 15-8 | **C9\_HCNT[15:8]** | C9 counter values (1) |
| 7-0 | **C9\_LCNT[7:0]** |
| 0x0038 |  | 15-0 | Reserved | Reserved for C10-C15 counter values |
| 0x0039 |  | 15-0 | Reserved |
| 0x003A |  | 15-0 | Reserved |
| 0x003B |  | 15-0 | Reserved |
| 0x003C |  | 15-0 | Reserved |
| 0x003D |  | 15-0 | Reserved |
| 0x003E | 0FFF |  | **Auto phase shift options** | |
|  | **AUTO\_PHCFG\_SMPLS** | Samples to compare in auto phase shift mode |
| 0x003F | 0002 |  | **AUTO\_PHCFG\_STEP** | Step size for auto phase |

Note 1: For detailed description see “Cyclone IV Device Handbook”, Chapter 5. Clock Networks and PLLs in Cyclone IV Devices.

### Registers of tstcfg module

Table 8 Register description of tstcfg module

| **Address** | **Def. value** | **Bits** | **Type** | **Name** | **Description** |
| --- | --- | --- | --- | --- | --- |
| 0x0060 | 00F0 |  | **SPI signature** | | |
| 15-8 |  | Reserved |  |
| 7-4 | R | **SPI\_SIGN\_REZULT** | Inverted bits from SPI\_SIGN register |
| 3-0 | R/W | **SPI\_SIGN** | SPI module test register. |
|  |  |  | **Test enable** | | |
| 0x0061 | 0000 | 15-6 |  | Reserved |  |
| 5 | R/W | **DDR2\_2\_TST\_EN** | DDR2\_2 memory test: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 4 | R/W | **DDR2\_1\_TST\_EN** | DDR2\_2 memory test: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 3 | R/W | **ADF\_TST\_EN** | Phase detector test: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 2 | R/W | **VCTCXO\_TST\_EN** | VCTCXO test: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 1 | R/W | **Si5351C\_TST\_EN** | Si5351C clock test: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 0 | R/W | **FX3\_PCLK\_TST\_EN** | FX3 PCLK clock test: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 0x0062 |  |  |  | Reserved |  |
| 0x0063 | 0000 |  | **Error insertion** | | |
| 15-6 |  | Reserved |  |
| 5 | R/W | **DDR2\_2\_TST\_FRC\_ERR** | DDR2\_2 insert error to memory test: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 4 | R/W | **DDR2\_1\_TST\_FRC\_ERR** | DDR2\_1 insert error to memory test: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 3 | R/W | **ADF\_TST\_FRC\_ERR** | Insert error to phase detector test: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 2 | R/W | **VCTCXO\_TST\_FRC\_ERR** | Insert error to VCTCXO test: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 1 | R/W | **Si5351C\_TST\_FRC\_ERR** | Insert error to Si5351C clock test: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 0 | R/W | **FX3\_PCLK\_TST\_FRC\_ERR** | Insert error to FX3 PCLK clock test: |
| 0 - Disabled **(Default)** |
| 1 - Enabled |
| 0x0064 |  |  |  | Reserved |  |
| 0x0065 | 0000 |  | **Test status** | | |
| 15-6 |  | Reserved |  |
| 5 | R | **DDR2\_2\_TST\_CMPLT** | DDR2\_2 test status: |
| 0 - Not completed |
| 1 - Completed |
| 4 | R | **DDR2\_1\_TST\_CMPLT** | DDR2\_1test status: |
| 0 - Not completed |
| 1 - Completed |
| 3 | R | **ADF\_TST\_CMPLT** | Phase detector test status: |
| 0 - Not completed |
| 1 - Completed |
| 2 | R | **VCTCXO\_TST\_CMPLT** | VCTCXO test status: |
| 0 - Not completed |
| 1 - Completed |
| 1 | R | **Si5351C\_TST\_CMPLT** | Si5351C clock test status: |
| 0 - Not completed |
| 1 - Completed |
| 0 | R | **FX3\_PCLK\_TST\_CMPLT** | FX3 PCLK clock test status: |
| 0 - Not completed |
| 1 - Completed |
| 0x0066 |  |  |  | Reserved |  |
|  |  |  | **Test results** | | |
| 0x0067 | 0000 | 15-6 |  | Reserved |  |
| 5 | R | **DDR2\_2\_TST\_REZ** | DDR2\_2 test result: |
| 0 - Fail |
| 1 - Pass |
| 4 | R | **DDR2\_1\_TST\_REZ** | DDR2\_1 test result: |
| 0 - Fail |
| 1 - Pass |
| 3 | R | **ADF\_TST\_REZ** | Not used |
| 2 | R | **VCTCXO\_TST\_REZ** | Not used |
| 1 | R | **Si5351C\_TST\_REZ** | Not used |
| 0 | R | **FX3\_PCLK\_TST\_REZ** | Not used |
|  |  |  | Clock test counter values | | |
| 0x0068 |  |  |  | Reserved |  |
| 0x0069 |  |  | R | **FX3\_CLK\_CNT** | FX3 PCLK clock counter value |
| 0x006A |  |  | R | **Si5351C\_CLK0\_CNT** | Si5351C CLK0 counter value |
| 0x006B |  |  | R | **Si5351C\_CLK1\_CNT** | Si5351C CLK1 counter value |
| 0x006C |  |  | R | **Si5351C\_CLK2\_CNT** | Si5351C CLK2 counter value |
| 0x006D |  |  | R | **Si5351C\_CLK3\_CNT** | Si5351C CLK3 counter value |
| 0x006E |  |  |  | Reserved |  |
| 0x006F |  |  | R | **Si5351C\_CLK5\_CNT** | Si5351C CLK5 counter value |
| 0x0070 |  |  | R | **Si5351C\_CLK6\_CNT** | Si5351C CLK6 counter value |
| 0x0071 |  |  | R | **Si5351C\_CLK7\_CNT** | Si5351C CLK7 counter value |
| 0x0072 |  |  | R | **LMK\_CLK\_CNT\_L** | LMK clock counter value |
| 0x0073 |  |  | R | **LMK\_CLK\_CNT\_H** |
| 0x0074 |  |  | R | **ADF\_CNT** | ADF transition count value |
| 0x0075 |  |  |  | Reserved |  |
|  |  |  | **DDR2\_1 detailed test results 1** | | |
| 0x0076 |  | 15-3 |  | Reserved |  |
| 2 | R | **DDR2\_1\_TST\_FAIL** | DDR2\_1 test result: |
| 0 - Test not completed |
| 1 - Fail |
| 1 | R | **DDR2\_1\_TST\_PASS** | DDR2\_1 test result: |
| 0 - Test not completed |
| 1 - Pass |
| 0 | R | **DDR2\_1\_TST\_CMPLT** | DDR2\_1 test result: |
| 0 - Test not completed |
| 1 - Test complete |
| 0x0077 |  |  | **DDR2\_1 detailed test results 2** | | |
| 15-0 | R | **DDR2\_1\_PNF\_PER\_BIT\_L** | DDR2\_1 data [15:0] bus pas not fail per bit: |
| 0 - Fail |
| 1 - Pass |
| 0x0078 |  |  | **DDR2\_1 detailed test results 3** | | |
| 15-0 | R | **DDR2\_1\_PNF\_PER\_BIT\_H** | DDR2\_1 data [31:16] bus pas not fail per bit: |
| 0 - Fail |
| 1 - Pass |
| 0x0079 |  | 15-0 |  | Reserved |  |
| 0x007A |  |  | **DDR2\_2 detailed test results 1** | | |
| 15-3 |  | Reserved |  |
| 2 | R | **DDR2\_2\_TST\_FAIL** | DDR2\_2 test result: |
| 0 - Test not completed |
| 1 - Fail |
| 1 | R | **DDR2\_2\_TST\_PASS** | DDR2\_2 test result: |
| 0 - Test not completed |
| 1 - Pass |
| 0 | R | **DDR2\_2\_TST\_CMPLT** | DDR2\_2 test result: |
| 0 - Test not completed |
| 1 - Test complete |
| 0x007B |  |  | **DDR2\_2 detailed test results 2** | | |
| 15-0 | R | **DDR2\_2\_PNF\_PER\_BIT\_L** | DDR2\_2 data [15:0] bus pas not fail per bit: |
| 0 - Fail |
| 1 - Pass |
| 0x007C |  |  | **DDR2\_2 detailed test results 3** | | |
| 15-0 | R | **DDR2\_2\_PNF\_PER\_BIT\_H** | DDR2\_2 data [31:16] bus pas not fail per bit: |
| 0 - Fail |
| 1 - Pass |
| 0x007D | AAAA |  | **TX test pattern 1** | | |
| 15-0 | R/W | **TX\_TST\_I** | TX test pattern I sample value |
| 0x007E | 5555 |  | **TX test pattern 2** | | |
| 15-0 | R/W | **TX\_TST\_Q** | TX test pattern Q sample value |
| 0x007F |  | 15-0 |  | Reserved |  |

### Registers of periphcfg module

Table 9 Register description of periphcfg module

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Address** | **Def. value** | **Bits** | **Type** | **Name** | **Description** |
| 0x00C0 | FFFF |  | **Board GPIO control 1** | | |
| 15-8 |  | Reserved |  |
| 7-0 | **R/W** | **BOARD\_GPIO\_OVRD** | GPIO control override (each bit controls corresponding GPIO): |
| 0 - Dedicated function |
| 1 - Overridden by user **(Default)** |
| 0x00C1 |  | 15-0 |  | Reserved for GPIO |  |
| 0x00C2 | 0000 |  | **Board GPIO control 2** | | |
| 15-8 |  | Reserved |  |
| 7-0 | **R** | **BOARD\_GPIO\_RD** | GPIO read value (each from corresponding GPIO): |
| 0 - Low level |
| 1 - High level |
| 0x00C3 |  | 15-0 |  | Reserved for GPIO |  |
| 0x00C4 | 0000 |  | **Board GPIO control 3** | | |
| 15-8 |  | Reserved |  |
| 7-0 | **R/W** | **BOARD\_GPIO\_DIR** | Onboard GPIO direction (each bit controls corresponding GPIO): |
| 0 - Input **(Default)** |
| 1 - Output |
| 0x00C5 |  | 15-0 |  | Reserved for GPIO |  |
| 0x00C6 | 0000 |  | **Board GPIO control 4** | | |
| 15-8 |  | Reserved |  |
| 7-0 | **R/W** | **BOARD\_GPIO\_VAL** | GPIO output value (each bit controls corresponding GPIO): |
| 0 - Low level |
| 1 - High level |
| 0x00C7 |  | 15-0 |  | Reserved for GPIO |  |
| 0x00C8 | 0000 | 15-0 |  | **PERIPH\_INPUT\_RD\_0** | Not used |
| 0x00C9 | 0000 | 15-0 |  | **PERIPH\_INPUT\_RD\_1** | Not used |
| 0x00CA |  | 15-0 |  | Reserved |  |
| 0x00CB |  | 15-0 |  | Reserved |  |
| 0x00CC | 0000 |  | **Board peripheral control 1** | | |
| 15-1 |  | **PERIPH\_OUTPUT\_OVRD\_0** | Not used |
| 0 | **R/W** | Fan control override: |
| 0 - Dedicated function **(Default)** |
| 1 - User controlled |
| 0x00CD | 0000 |  | **Board peripheral control 1** | | |
| 15-1 |  | **PERIPH\_OUTPUT\_VAL\_0** | Not used |
| 0 | **R/W** | Fan control pin: |
| 0 - OFF **(Default)** |
| 1- ON |
| 0x00CE | 0000 | 15-0 |  | **PERIPH\_OUTPUT\_OVRD\_1** | Not used |
| 0x00CF | 0000 | 15-0 |  | **PERIPH\_OUTPUT\_VAL\_1** | Not used |
| 0x00D0 |  | 15-0 |  | Reserved |  |
| 0x00D1 |  | 15-0 |  | Reserved |  |
| 0x00D2 |  | 15-0 |  | Reserved |  |
| 0x00D3 |  | 15-0 |  | Reserved |  |
| 0x00D4 |  | 15-0 |  | Reserved |  |
| 0x00D5 |  | 15-0 |  | Reserved |  |
| 0x00D6 |  | 15-0 |  | Reserved |  |
| 0x00D7 |  | 15-0 |  | Reserved |  |
| 0x00D8 |  | 15-0 |  | Reserved |  |
| 0x00D9 |  | 15-0 |  | Reserved |  |
| 0x00DA |  | 15-0 |  | Reserved |  |
| 0x00DB |  | 15-0 |  | Reserved |  |
| 0x00DC |  | 15-0 |  | Reserved |  |
| 0x00DD |  | 15-0 |  | Reserved |  |
| 0x00DE |  | 15-0 |  | Reserved |  |
| 0x00DF |  | 15-0 |  | Reserved |  |

## FX3 Slave FIFO interface – FX3\_slaveFIFO5b

Provides data transfer between external FX3 SuperSpeed USB 3.0 peripheral controller and FPGA trough GPIF II interface (See <http://www.cypress.com/part/cyusb3014-bzxi> for documentation).

All data exchange between slaveFIFO5b module and other FPGA logic is done through FIFO buffers. Module slaveFIFO5b constantly monitors GPIF II status flags and all FIFO buffers. For example, internal logic writes IQ stream packets containing 4kB data to FIFO buffer through EP81 ports. Once slave FIFO5b module detects that EP81 FIFO buffers contains 4kB data and GPIF II flags indicate that FX3 controller is ready, all data is read from FIFO buffer and written to FX3 controller trough GPIF interface.



Figure 4 FX3\_slaveFIFO5b block diagram

Table 10 Description of FX3\_slaveFIFO5b instances

| **Instance** | **Description** |
| --- | --- |
| SlaveFIFO5b | Provides data transfer between GPIF II interface and internal FIFO buffers. |
| fifo\_inst (EP81) | Stream endpoint FIFO buffer of 16kB size. |
| fifo\_inst (EP01\_0) | Stream endpoint FIFO buffer of 4kB size. |
| fifo\_inst (EP01\_1) | Stream endpoint FIFO buffer of 4kB size. |
| fifo\_inst (EP8F) | Control endpoint FIFO buffer of 1kB size. |
| fifo\_inst (EP0F) | Control endpoint FIFO buffer of 0.5kB size. |

Table 11 FX3\_slaveFIFO5b module parameters

| **Parameter** | **Type** | **Default** | **Description** |
| --- | --- | --- | --- |
| Start address of SPI registers | | | |
| dev\_family | string | Cyclone IV E | Device family name |
| data\_width | integer | 32 | GPIF II interface data width |
| Stream, socket 0, (PC->FPGA) | | | |
| EP01\_0\_rdusedw\_width | integer | 9 | EP01\_0 FIFO read used words size (29-1= 256 words) |
| EP01\_0\_rwidth | integer | 128 | EP01\_0 FIFO read word size |
| EP01\_1\_rdusedw\_width | integer | 11 | EP01\_1 FIFO read used words size (211-1= 1024 words) |
| EP01\_1\_rwidth | integer | 32 | EP01\_1 FIFO read word size |
| Stream, socket 2, (FPGA->PC) | | | |
| EP81\_wrusedw\_width | integer | 12 | EP81 FIFO write used words size (212-1= 2048 words) |
| EP81\_wwidth | integer | 64 | EP81 FIFO write word size |
| Control, socket 1, (PC->FPGA) | | | |
| EP0F\_rdusedw\_width | integer | 8 | EP0F FIFO read used words size (28-1= 128 words) |
| EP0F\_rwidth | integer | 32 | EP0F FIFO read word size |
| Control, socket 3, (FPGA->PC) | | | |
| EP8F\_wrusedw\_width | integer | 9 | EP8F FIFO write used words size (29-1= 256 words) |
| EP8F\_wwidth | integer | 32 | EP8F FIFO write word size |

Table 12 FX3\_slaveFIFO5B module ports

| **Port** | **Type** | **Width** | **Description** |
| --- | --- | --- | --- |
| reset\_n | in | 1 | Reset active low |
| clk | in | 1 | Clock 100 Mhz |
| usb\_speed | in | 1 | USB speed select 0 - USB2.0, 1- USB3.0. |
| FX3 GPIF II interface | | | |
| slcs | out | 1 | Chip select |
| fdata | inout | 32 | Data |
| faddr | out | 5 | FIFO address |
| slrd | out | 1 | Read select |
| sloe | out | 1 | Output enable |
| slwr | out | 1 | Write select |
| flaga | in | 1 |  |
| flagb | in | 1 |  |
| flagc | in | 1 | Not used in |
| flagd | in | 1 | Not used in |
| pktend | out | 1 | Packet end |
| EPSWITCH | out | 1 | Not used |
| EP01 buffer select | | | |
| EP01\_sel | in | 1 | 0 - EP01\_0, 1 - EP01\_1 |
| Stream endpoint FIFO 0 (PC->FPGA) | | | |
| EP01\_0\_rdclk | in | 1 | Read clock |
| EP01\_0\_aclrn | in | 1 | Asynchronous clear, active low |
| EP01\_0\_rd | in | 1 | Read request |
| EP01\_0\_rdata | out | EP01\_0\_rwidth | Read data |
| EP01\_0\_rempty | out | 1 | Read empty |
| EP01\_0\_rdusedw | out | EP01\_0\_rdusedw\_width | Red used words |
| Stream endpoint FIFO 1 (PC->FPGA) | | | |
| EP01\_1\_rdclk | in | 1 | Read clock |
| EP01\_1\_aclrn | in | 1 | Asynchronous clear, active low |
| EP01\_1\_rd | in | 1 | Read request |
| EP01\_1\_rdata | out | EP01\_1\_rwidth | Read data |
| EP01\_1\_rempty | out | 1 | Read empty |
| EP01\_1\_rdusedw | out | EP01\_1\_rdusedw\_width | Red used words |
| Stream endpoint FIFO (FPGA->PC) | | | |
| EP81\_wclk | in | 1 | Write clock |
| EP81\_aclrn | in | 1 | Asynchronous clear, active low |
| EP81\_wr | in | 1 | Write request |
| EP81\_wdata | in | EP81\_wwidth | Write data |
| EP81\_wfull | out | 1 | Write full |
| EP81\_wrusedw | out | EP81\_wrusedw\_width | Write used words |
| Control endpoint FIFO (PC->FPGA) | | | |
| EP0F\_rdclk | in | 1 | Read clock |
| EP0F\_aclrn | in | 1 | Asynchronous clear, active low |
| EP0F\_rd | in | 1 | Read request |
| EP0F\_rdata | out | EP0F\_rwidth | Read data |
| EP0F\_rempty | out | 1 | Read empty |
| Control endpoint FIFO (FPGA->PC) | | | |
| EP8F\_wclk | in | 1 | Write clock |
| EP8F\_aclrn | in | 1 | Asynchronous clear, active low |
| EP8F\_wr | in | 1 | Write request |
| EP8F\_wdata | in | EP8F\_wwidth | Write data |
| EP8F\_wfull | out | 1 | Write full |
| Status | | | |
| GPIF\_busy | out | 1 | std\_logic |

## LMS7002 Receive and transmit interface – rxtx\_top

Main function of rxtx\_top module is for receive and transmit IQ samples from/to LMS7002 chip and provide IQ sample synchronization. See **Figure 5** for block diagram and **Table 13** for instance description.



Figure 5 rxtx\_top block diagram

Table 13 Description of rxtx\_top instances

| **Instance** | **Description** |
| --- | --- |
| tx\_path\_top | Transmit logic. See **3.5.2 Transmit interface – tx\_path\_top**. |
| wfm\_player | Waveform player for LMS\_DIQ1 interface |
| txiqmux | Mux for tx\_path\_top and wfm\_player modules |
| rx\_path\_top | Receive logic. See **3.5.1 Receive interface – rx\_path\_top**. |

Table 14 rxtx\_top parameters description

| **Parameter** | **Type** | **Default** | **Description** |
| --- | --- | --- | --- |
| DEV\_FAMILY | string | Cyclone IV E | Device family |
| TX parameters | | | |
| TX\_IQ\_WIDTH | integer | 12 | TX IQ sample width |
| TX\_N\_BUFF | integer | 4 | TX number of buffers, 2,4 valid values |
| TX\_IN\_PCT\_SIZE | integer | 4096 | TX packet size in bytes |
| TX\_IN\_PCT\_HDR\_SIZE | integer | 16 | TX packet header size in bytes |
| TX\_IN\_PCT\_DATA\_W | integer | 128 | TX packet read data width |
| TX\_IN\_PCT\_RDUSEDW\_W | integer | 11 | TX packet read used words width |
| TX\_OUT\_PCT\_DATA\_W | integer | 64 | TX output packet data width |
| RX parameters | | | |
| RX\_IQ\_WIDTH | integer | 12 | RX IQ sample width |
| RX\_INVERT\_INPUT\_CLOCKS | string | ON | Clock invert option on LMS\_DIQ2 interface |
| RX\_SMPL\_BUFF\_RDUSEDW\_W | integer | 11 | RX sample buffer read used words width. Words=211-1 |
| RX\_PCT\_BUFF\_WRUSEDW\_W | integer | 12 | RX packet buffer read used words width. Words=212-1 |
| WFM | | | |
| WFM\_IN\_PCT\_DATA\_W | integer | 32 | WFM in packet read data width |
| WFM\_IN\_PCT\_RDUSEDW\_W | integer | 11 | WFM in packet read used words width. Words= 211-1 |
| DDR2 controller parameters | | | |
| WFM\_CNTRL\_RATE | integer | 1 | 1 - full rate, 2 - half rate |
| WFM\_CNTRL\_BUS\_SIZE | integer | 16 | DDR2 memory data width |
| WFM\_ADDR\_SIZE | integer | 25 | DDR2 memory address width |
| WFM\_LCL\_BUS\_SIZE | integer | 64 | DDR2 controller local data bus size |
| WFM\_LCL\_BURST\_LENGTH | integer | 2 | DDR2 controller local burst length |
| WFM player parameters | | | |
| WFM\_WFM\_INFIFO\_SIZE | integer | 12 | WFM in FIFO buffer write used words width. Words= 212-1 |
| WFM\_DATA\_WIDTH | integer | 32 | WFM data width |
| WFM\_IQ\_WIDTH | integer | 12 | WFM IQ sample width |

| **Port** | **Type** | **Width** | **Description** |
| --- | --- | --- | --- |
| Configuration memory ports | | | |
| from\_fpgacfg | in | t\_FROM\_FPGACFG; | Configuration registers bus |
| to\_tstcfg\_from\_rxtx | out | t\_TO\_TSTCFG\_FROM\_RXTX; |
| from\_tstcfg | in | t\_FROM\_TSTCFG; |
| TX path | | | |
| tx\_clk | in | 1 | TX interface clock |
| tx\_clk\_reset\_n | in | 1 | TX interface reset, active low |
| tx\_pct\_loss\_flg | out | 1 | TX packet loss flag, 0 - No packet loss, 1 - Packet lost. |
| tx\_txant\_en | out | 1 | TX transmit flag. 0 - No transmission, 1 - TX is transmitting samples |
| TX interface data | | | |
| tx\_DIQ | out | TX\_IQ\_WIDTH | TX samples |
| tx\_fsync | out | 1 | TX sync signal |
| TX FIFO read ports | | | |
| tx\_in\_pct\_reset\_n\_req | out | 1 | TX packet buffer reset request, active low |
| tx\_in\_pct\_rdreq | out | 1 | TX packet buffer read request |
| tx\_in\_pct\_data | in | TX\_IN\_PCT\_DATA\_W | TX packet buffer read data |
| tx\_in\_pct\_rdempty | in | 1 | TX packet buffer read empty |
| tx\_in\_pct\_rdusedw | in | TX\_IN\_PCT\_RDUSEDW\_W | TX packet buffer read used words |
| WFM Player | | | |
| wfm\_pll\_ref\_clk | in | 1 | Reference clock for DDR2 controller |
| wfm\_pll\_ref\_clk\_reset\_n | in | 1 | Reset for DDR2 controller, active low. |
| wfm\_phy\_clk | out | 1 | DDR2 controller local interface clock output |
| WFM FIFO read ports | | | |
| wfm\_in\_pct\_reset\_n\_req | out | 1 | WFM packet buffer reset request, active low |
| wfm\_in\_pct\_rdreq | out | 1 | WFM packet buffer read request |
| wfm\_in\_pct\_data | in | WFM\_IN\_PCT\_DATA\_W | WFM packet buffer read data |
| wfm\_in\_pct\_rdempty | in | 1 | WFM packet buffer read empty |
| wfm\_in\_pct\_rdusedw | in | WFM\_IN\_PCT\_RDUSEDW\_W | WFM packet buffer read used words |
| DDR2 external memory signals | | | |
| wfm\_mem\_odt | out | 1 | [External memory interface](https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/ug/ug_altmemphy.pdf) |
| wfm\_mem\_cs\_n | out | 1 |
| wfm\_mem\_cke | out | 1 |
| wfm\_mem\_addr | out | 13 |
| wfm\_mem\_ba | out | 3 |
| wfm\_mem\_ras\_n | out | 1 |
| wfm\_mem\_cas\_n | out | 1 |
| wfm\_mem\_we\_n | out | 1 |
| wfm\_mem\_dm | out | 2 |
| wfm\_mem\_clk | inout | 1 |
| wfm\_mem\_clk\_n | inout | 1 |
| wfm\_mem\_dq | inout | 16 |
| wfm\_mem\_dqs | inout | 2 |
| RX path | | | |
| rx\_clk | in | 1 | RX interface clock |
| rx\_clk\_reset\_n | in | 1 | RX interface reset, active low |
| Rx interface data | | | |
| rx\_DIQ | in | RX\_IQ\_WIDTH | RX IQ samples |
| rx\_fsync | in | 1 | RX IQ sync signal |
| Packet fifo ports | | | |
| rx\_pct\_fifo\_aclrn\_req | out | 1 | RX packet buffer reset request, active low |
| rx\_pct\_fifo\_wusedw | in | RX\_PCT\_BUFF\_WRUSEDW\_W | RX packet buffer write used words |
| rx\_pct\_fifo\_wrreq | out | 1 | RX packet buffer write request |
| rx\_pct\_fifo\_wdata | out | 64 | RX packet buffer write data |
| Sample compare | | | |
| rx\_smpl\_cmp\_start | in | 1 | RX interface sample compare. 0 - disabled, 1-enabled |
| rx\_smpl\_cmp\_length | in | 16 | RX interface number of samples to compare. |
| rx\_smpl\_cmp\_done | out | 1 | RX interface sample compare done. 0 - not done, 1-done |
| rx\_smpl\_cmp\_err | out | 1 | RX interface sample compare status. 0 - no error, 1 - error |

### Receive interface – rx\_path\_top

Once rx\_path\_top **Figure 6** is enabled diq2fifo and data2packets modules starts continuously packing IQ samples into 4kB packets. For packet structure see [Stream protocol](https://github.com/myriadrf/LimeSuite/blob/master/docs/StreamProtocol.pdf) document.

Packets are written to 16kB EP81 FIFO buffer to maintain continuous data flow in short periods when USB3.0 host cannot accept data. If USB3.0 host halts data transfer for longer time period and four packets are buffered into 16kB buffer, FIFO full condition arises and other packets are dropped. When host starts to receive data after FIFO full condition, host should expect to receive those four buffered packets.

Module rx\_path\_top provides two 64bit sample counters. One is for TX logic – tx\_path\_top. TX logic uses this counter to synchronize transmitted LMS\_DQ1 samples with received LMS\_DIQ2 samples. Other is used for LMS\_DI2 samples packing into 4kB packets.

When rx\_path\_top is enabled diq2fifo module starts to collect IQ samples from LMS\_DIQ2 bus, collected samples are written to FIFO buffer and each write enables smpl\_cnt:inst4 module to increase its counter value. This means that counter value increases in same continuous rate as IQ sample rate.

Module smpl\_cnt:inst3 is used for LMS\_DI2 samples packing into 4kB packets. Module data2packets reads IQ samples in bursts from FIFO buffer, each read enables smpl\_cnt:inst3 module to increase its counter value. One read burst fills one 4kB packet and there are some idle cycles between bursts.



Figure 6 rx\_path\_top block diagram

Table 15 rx\_path\_top inctance description

| **Instance** | **Description** |
| --- | --- |
| diq2fifo | Captures IQ samples and writes to FIFO buffer. |
| fifo\_inst | FIFO buffer for storing samples. |
| data2packets | Module for packing IQ samples to 4kB packets. |
| smpl\_cnt:inst3 | Sample counter for tx\_path\_top. |
| smpl\_cnt:inst4 | Sample counter for data2packets module. |

### Transmit interface – tx\_path\_top

Transmit module tx\_path\_top reads IQ samples from EP01\_0 FIFO buffer packed in 4kB packets. Packet header (see [Stream protocol](https://github.com/myriadrf/LimeSuite/blob/master/docs/StreamProtocol.pdf) document) contains sample number (or so-called time stamp) at which packet should be transmitted.

By using sample numbers from rx\_path\_top and received sample numbers in packet header transmitted IQ samples can be synchronized with received IQ samples.

Module p2d\_wr\_fsm separates packet header and payload. Packet payload is written into one of four 4kB FIFO buffers located in packets2data module and packet header is stored in p2d\_rd module. This module can work in two modes:

* **Synchronization enabled** - module compares received sample number from packet header and sample number from rx\_path\_top. When sample number from received packet is equal to sample number of rx\_path\_top module (this means that it is time to send TX packet), read process begins and IQ samples are transmitted to LMS\_DIQ1 interface. When sample number from received packet is greater than sample number of rx\_path\_top module (this means that received packet should be sent after some time) p2d\_rd waits until those sample number will be equal. When sample number from received packet is less than sample number of rx\_path\_top module (this means that packet arrived to late) corresponding FIFO buffer is cleared.
* **Synchronization disabled** – module does not compare sample numbers and every received packet is transmitted to LMS\_DIQ1 interface.

Block diagram can be found in **Figure 7** and instance description in **Table 16**.



Figure 7 tx\_path\_top block diagram

Table 16 tx\_path\_top instance description

| **Instance** | **Description** |
| --- | --- |
| packets2data\_top | Wrapper file |
| packets2data | Wrapper file |
| p2d\_wr\_fsm | Module reads packets from EP01\_0 buffer and places to one of the 4kB FIFO buffers in increasing order and stores corresponding sample number from packet header. |
| p2d\_rd | Module checks one of the FIFO buffers if it is filled with samples in increasing order. When buffer is ready depending on received sample number from packet header and sample number from rx\_path\_top module buffer can be cleared or IQ sample reading begins. |
| fifo\_inst | FIFO buffer |
| fifo2diq | Module reads samples from FIFO buffer and writes to LMS\_DIQ1 interface. |
| sync\_fifo\_rw | Dual clock FIFO buffer for clock domain crossing. |
| bit\_unpack\_64 | Depending on mode selection samples are unpacked (see [Stream protocol](https://github.com/myriadrf/LimeSuite/blob/master/docs/StreamProtocol.pdf) document). |

### Waveform player – wfm\_player\_top

Waveform player – wfm\_player\_top can be used to load waveform from EP01\_1 endpoint to external DDR2 memory and played back to LMS\_DIQ1 interface. Samples can be loaded using 4kB packets (see [Stream protocol](https://github.com/myriadrf/LimeSuite/blob/master/docs/StreamProtocol.pdf) document). External memory can store 128MB of data. Block diagram can be found in **Figure 8**.

When loading waveform for LMS\_DIQ1 channels (MIMO mode) waveforms should be same length.



Figure 8 wfm\_player\_top block diagram

Table 17 wfm\_player\_top instance description

| **Instance** | **Description** |
| --- | --- |
| wfm\_player | Waveform player instance, reads IQ packets from EP01\_1 FIFO buffer and writes to DDR2\_ctrl module. |
| DDR2\_ctrl | External DDR2 memory controller. |
| decompress | Decompress IQ samples. |
| rd\_tx\_fifo | Reads decompressed samples and writes to LMS\_DIQ1 interface. |

## General periphery – general\_periph\_top

General periphery - general\_periph\_top module is responsible for controlling on board periphery such as LED, GPIO and Fan, default functions can be found in **Table 18**. Also default function can be overridden by internal registers see chapter **3.3 Softcore processor – nios\_cpu**.

Table 18 Default functions of LEDS, GPIO and fan

| **Schematic name** | **Board label** | **Type** | **Description** |
| --- | --- | --- | --- |
| FPGA\_LED1 | FPGA1 | Clock status | Blinking indicates presence of TCXO clock.  Colour indicates status of FPGA PLLs that are used for LMS digital interface clocking: Green – both PLLs are locked; Red/Green – at least one PLL is not locked. |
| FPGA\_LED2 | FPGA2 | TCXO control mode | No light – TCXO is controlled from DAC  Red – TCXO is controlled from phase detector and is not locked to external reference clock Green – TCXO is controlled from phase detector and is locked to external reference clock |
| FX3\_LED | FX3 | USB activity | USB3.0 (FX3) controller, slave FIFO (GPIF) interface module and NIOS CPU activity indication:  Green – idle, Red – busy. |
| FPGA\_GPIO0 | FPGA\_GPIO |  | Indicates when TX is transmitting IQ samples. 0 – not transmitting, 1 – transmitting. |
| FPGA\_GPIO1 |  | Indicates RXPLL lock status. 0 – no lock, 1 - locked |
| FPGA\_GPIO2 |  | Indicates TXPLL lock status. 0 – no lock, 1 - locked |
| FPGA\_GPIO3 |  | Indicates TX packet loss, 0 – no loss, 1 – packet lost. |
| FPGA\_GPIO4 |  | - |
| FPGA\_GPIO5 |  | - |
| FPGA\_GPIO6 |  | - |
| FPGA\_GPIO7 |  | - |
| FAN\_CTRL | FAN |  | Fan control pin. Connected to LM75\_OS temperature sensor pin. |

Block diagram can be found in **Figure 9**, instances are described in **Table 19**. See **Table 20** and **Table 21** for module parameters and port description.



Figure 9 Module general\_periph\_top block diagram

Table 19 Module instance description

| **Instance** | **Description** |
| --- | --- |
| alive | Basic counter to implement blinking on led1. |
| FPGA\_LED1\_cntrl | Led1 control module, for showing clock status |
| FPGA\_LED2\_cntrl | Led2 control module, for showing TCXO control mode |
| FX3\_LED\_cntrl | Led3 control module, for USB and NIOS CPU activity. |
| periphcfg | SPI register instance, provides control for gpio\_ctrl instance and fan. |
| gpio\_ctrl | GPIO control instance |

Table 20 Module general\_periph\_top parameters

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | **Type** | **Default** | **Description** |
| DEV\_FAMILY | string | "CYCLONE IV E" | FPGA device family name |
| N\_GPIO | integer | 8 | Number of GPIO used |

Table 21 Module general\_periph\_top input and output port description

| **Port** | **Type** | **Width** | **Description** |
| --- | --- | --- | --- |
| clk | in | 1 | Free running clock |
| reset\_n | in | 1 | Asynchronous, active low reset |
| SPIregisters(Default address range 0x00C0-0x00DF) | | | |
| periphcfg\_maddress | in | 10 | Address of SPI slave registers |
| periphcfg\_sdin | in | 1 | SPI slave datain |
| periphcfg\_sclk | in | 1 | SPI slave clock |
| periphcfg\_sen | in | 1 | SPI slave select |
| periphcfg\_sdout | out | 1 | SPI slave dataout |
| LED1(Clock and PLL lock status) | | | |
| led1\_pll1\_locked | in | 1 | Lock status from PLL1 |
| led1\_pll2\_locked | in | 1 | Lock status from PLL2 |
| led1\_ctrl | in | 3 | led1\_ctrl[0]–manual LED control enable; led1\_ctrl[1]–red LED enable in manual mode; led1\_ctrl[2]–green LED enable in manual mode; |
| led1\_g | out | 1 | Output to dual colour LED1 pin |
| led1\_r | out | 1 | Output to dual colour LED1 pin |
| LED2(TCXO control status) | | | |
| led2\_clk | in | 1 | Clock from SPI master connected to DAC and ADF |
| led2\_adf\_muxout | in | 1 | Multiplexer output from ADF4002 |
| led2\_dac\_ss | in | 1 | DAC slave select |
| led2\_adf\_ss | in | 1 | ADF slave select |
| led2\_ctrl | in | 3 | led2\_ctrl[0]–manual LED control enable; led2\_ctrl[1]–red LED enable in manual mode; led2\_ctrl[2]–green LED enable in manual mode; |
| led2\_g | out | 1 | Output to dual colour LED2 pin |
| led2\_r | out | 1 | Output to dual colour LED2 pin |
| LED3(FX3 and NIOS CPU busy) | | | |
| led3\_g\_in | in | 1 | Green LED input |
| led3\_r\_in | in | 1 | Red LED input |
| led3\_ctrl | in | 3 | led3\_ctrl[0]–manual LED control enable; led3\_ctrl[1]–red LED enable in manual mode; Led3\_ctrl[2]–green LED enable in manual mode; |
| led3\_hw\_ver | in | 4 | Hardware version input pins |
| led3\_g | out | 1 | Output to dual colour LED3 pin |
| led3\_r | out | 1 | Output to dual colour LED3 pin |
| GPIO | | | |
| gpio\_dir | in | N\_GPIO | GPIO direction control, 0 – input, 1 – output |
| gpio\_out\_val | in | N\_GPIO | GPIO output value when direction is set to output |
| gpio\_rd\_val | out | N\_GPIO | GPIO input value when direction is set to input |
| gpio | inout | N\_GPIO | Connected to GPIO pins |
| Fan control | | | |
| fan\_sens\_in | in | 1 | From temperature sensor |
| fan\_ctrl\_out | out | 1 | To Fan control output |

## PLL module – pll\_top

PLL module – pll\_top (**Figure 10)** provides required clock sources for LM7002 RX and TX digital interfaces. Inside this module there are two dynamically reconfigurable PLL instances **Figure 11**. Clock frequency and phase relationship can be changed while FPGA is in user mode. Instance description can be found in **Table 22**.



Figure 10 PLL module – pll\_top



Figure 11 tx\_pll\_top/rx\_pll\_top modules

Table 22. pll\_top module instance description

| **Instance** | **Description** |
| --- | --- |
| pllcfg\_top | PLL configuration control module |
| tx\_pll\_top | PLL dedicated for TX interface |
| rx\_pll\_top | PLL dedicated for RX interface |

Table 23. pll\_top module parameters

| **Parameter** | **Type** | **Default** | **Description** |
| --- | --- | --- | --- |
| N\_PLL | integer | 2 |  |
| TX PLL parameters | | | |
| TXPLL\_BANDWIDTH\_TYPE | string | "AUTO" | PLL bandwidth setting |
| TXPLL\_CLK0\_DIVIDE\_BY | natural | 1 | PLL c0 output division factor |
| TXPLL\_CLK0\_DUTY\_CYCLE | natural | 50 | PLL c0 output duty cycle |
| TXPLL\_CLK0\_MULTIPLY\_BY | natural | 1 | PLL c0 multiplication factor |
| TXPLL\_CLK0\_PHASE\_SHIFT | string | "0" | PLL c0 phase shift setting in degrees |
| TXPLL\_CLK1\_DIVIDE\_BY | natural | 1 | PLL c1 output division factor |
| TXPLL\_CLK1\_DUTY\_CYCLE | natural | 50 | PLL c1 output duty cycle |
| TXPLL\_CLK1\_MULTIPLY\_BY | natural | 1 | PLL c1 multiplication factor |
| TXPLL\_CLK1\_PHASE\_SHIFT | string | "0" | PLL c0 phase shift setting in degrees |
| TXPLL\_COMPENSATE\_CLOCK | string | "CLK1" | Specifies for which PLL output delay compensation is done |
| TXPLL\_INCLK0\_INPUT\_FREQUENCY | natural | 6250 | TX PLL input frequency period in ps |
| TXPLL\_INTENDED\_DEVICE\_FAMILY | string | "Cyclone IV E" | FPGA device family |
| TXPLL\_OPERATION\_MODE | string | "SOURCE\_ SYNCHRONOUS" | PLL compensation mode setting |
| TXPLL\_SCAN\_CHAIN\_MIF\_FILE | string | "ip/txpll/pll.mif" | PLL memory initialization file location |
| TXPLL\_DRCT\_C0\_NDLY | integer | 1 | Number of logic cells in c0 TX PLL output when PLL is bypassed |
| TXPLL\_DRCT\_C1\_NDLY | integer | 2 | Number of logic cells in TX PLL c1 output when PLL is bypassed |
| RX PLL parameters | | | |
| RXPLL\_BANDWIDTH\_TYPE | string | "AUTO" | PLL bandwidth setting |
| RXPLL\_CLK0\_DIVIDE\_BY | natural | 1 | PLL c0 output division factor |
| RXPLL\_CLK0\_DUTY\_CYCLE | natural | 50 | PLL c0 output duty cycle |
| RXPLL\_CLK0\_MULTIPLY\_BY | natural | 1 | PLL c0 multiplication factor |
| RXPLL\_CLK0\_PHASE\_SHIFT | string | "0" | PLL c0 phase shift setting in degrees |
| RXPLL\_CLK1\_DIVIDE\_BY | natural | 1 | PLL c1 output division factor |
| RXPLL\_CLK1\_DUTY\_CYCLE | natural | 50 | PLL c1 output duty cycle |
| RXPLL\_CLK1\_MULTIPLY\_BY | natural | 1 | PLL c1 multiplication factor |
| RXPLL\_CLK1\_PHASE\_SHIFT | string | "0" | PLL c0 phase shift setting in degrees |
| RXPLL\_COMPENSATE\_CLOCK | string | "CLK1" | Specifies for which PLL output delay compensation is done |
| RXPLL\_INCLK0\_INPUT\_FREQUENCY | natural | 6250 | RX PLL input frequency period in ps |
| RXPLL\_INTENDED\_DEVICE\_FAMILY | string | "Cyclone IV E" | FPGA device family |
| RXPLL\_OPERATION\_MODE | string | "SOURCE\_ SYNCHRONOUS" | PLL compensation mode setting |
| RXPLL\_SCAN\_CHAIN\_MIF\_FILE | string | "ip/pll/pll.mif" | PLL memory initialization file location |
| RXPLL\_DRCT\_C0\_NDLY | integer | 1 | Number of logic cells in RX PLL c0 output when PLL is bypassed |
| RXPLL\_DRCT\_C1\_NDLY | integer | 2 | Number of logic cells in RX PLL c1 output when PLL is bypassed |
|  |  |  |  |

Table 24 pll\_top port description

| **Port** | **Type** | **Width** | **Description** |
| --- | --- | --- | --- |
| TX PLL ports | | | |
| txpll\_inclk | in | 1 | PLL input clock from LMS\_MCLK1 pin |
| txpll\_reconfig\_clk | in | 1 | Free running clock, used for PLL reconfiguration. |
| txpll\_logic\_reset\_n | in | 1 | PLL logic active low reset. |
| txpll\_c0 | out | 1 | TX PLL c0 output clock |
| txpll\_c1 | out | 1 | TX PLL c1 output clock (phase shifted version of c0) |
| txpll\_locked | out | 1 | TX PLL lock status. Outputs high level vhen PLL is locked |
| txpll\_smpl\_cmp\_en | out | 1 | Sample compare enable. Used in auto phase searching mode. |
| txpll\_smpl\_cmp\_done | in | 1 | Sample compare done indication. Used in auto phase searching mode. |
| txpll\_smpl\_cmp\_error | in | 1 | Sample compare error status. Used in auto phase searching mode. |
| txpll\_smpl\_cmp\_cnt | out | 16 | Number of samples to be checked. Used in auto phase searching mode |
| RX PLL ports | | | |
| rxpll\_inclk | in | 1 | PLL input clock from LMS\_MCLK2 pin |
| rxpll\_reconfig\_clk | in | 1 | Free running clock, used for PLL reconfiguration. |
| rxpll\_logic\_reset\_n | in | 1 | PLL logic active low reset. |
| rxpll\_c0 | out | 1 | RX PLL c0 output clock |
| rxpll\_c1 | out | 1 | RX PLL c1 output clock (phase shifted version of c0) |
| rxpll\_locked | out | 1 | RX PLL lock status. Outputs high level vhen PLL is locked |
| rxpll\_smpl\_cmp\_en | out | 1 | Sample compare enable. Used in auto phase searching mode. |
| rxpll\_smpl\_cmp\_done | in | 1 | Sample compare done indication. Used in auto phase searching mode. |
| rxpll\_smpl\_cmp\_error | in | 1 | Sample compare error status. Used in auto phase searching mode. |
| rxpll\_smpl\_cmp\_cnt | out | 16 | Number of samples to be checked. Used in auto phase searching mode |
| pllcfg ports | | | |
| pllcfg\_in | in | 1 | Configuration register bus |
| pllcfg\_out | out | 1 |

## Board test module – tst\_top

Board test module – tst\_top **Figure 12** is used to test clock inputs and DDR2 memory. Separate tests can be enabled and results can be read from internal registers see **3.3.3 Registers of tstcfg module**. Module port description can be found in **Table 25**.



Figure 12 tst\_top block diagram

Table 25 tst\_top module port description

|  |  |  |  |
| --- | --- | --- | --- |
| **Port** | **Type** | **Width** | **Description** |
| FX3\_clk | in | 1 | 100MHz reference clock |
| reset\_n | in | 1 | Reset, active low |
| Clock inputs | | | |
| Si5351C\_clk\_0 | in | 1 | Clock inputs form clock generator Si5351C |
| Si5351C\_clk\_1 | in | 1 |
| Si5351C\_clk\_2 | in | 1 |
| Si5351C\_clk\_3 | in | 1 |
| Si5351C\_clk\_5 | in | 1 |
| Si5351C\_clk\_6 | in | 1 |
| Si5351C\_clk\_7 | in | 1 |
| LMK\_CLK | in | 1 | Clock buffer |
| ADF\_MUXOUT | in | 1 | Phase detector mux output |
| DDR2 external memory signals | | | |
| mem\_pllref\_clk | in | 1 | [External memory interface](https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/ug/ug_altmemphy.pdf) |
| mem\_odt | out | 1 |
| mem\_cs\_n | out | 1 |
| mem\_cke | out | 1 |
| mem\_addr | out | 13 |
| mem\_ba | out | 3 |
| mem\_ras\_n | out | 1 |
| mem\_cas\_n | out | 1 |
| mem\_we\_n | out | 1 |
| mem\_dm | out | 2 |
| mem\_clk | inout | 1 |
| mem\_clk\_n | inout | 1 |
| mem\_dq | inout | 16 |
| mem\_dqs | inout | 2 |
| To configuration memory | | | |
| to\_tstcfg | out | t\_TO\_TSTCFG | Configuration bus |
| from\_tstcfg | in | t\_FROM\_TSTCFG |

# Examples

In this chapter various examples can be found on how to use gateware.

## Accessing FPGA registers

Internal FPGA registers can be accessed using USB3.0 host via EP0F and EP8F endpoints. See **LMS64C\_protocol** document for protocol structure and description of commands used in examples. See chapter **3.3 Softcore processor – nios\_cpu** for internal FPGA register description.

**Read** – 64byte packet containing request command “CMD\_BRDSPI16\_RD” has to be sent to EP0F endpoint and 64 bytes response packet has to be read from EP8F endpoint. Read example reads 0x0000 address Board\_ID register value, which is 0x000E for LimeSDR-USB board.

Request – USB3.0 writes 64B to EP0F:

Address

0000 56 00 01 00 00 00 00 00 00 00 00 00 00 00 00 00

0010 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

0020 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

0030 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

Response – USB3.0 host reads 64B from EP8F:

Address

0000 56 01 01 00 00 00 00 00 00 00 00 0E 00 00 00 00

0010 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

0020 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

0030 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

**Write** – 64byte packet containing request command “CMD\_BRDSPI16\_WR” has to be sent to EP0F endpoint and 64 bytes response packet has to be read from EP8F endpoint. Write example writes 0x1234 value to 0x00DF address. This register is currently reserved and has no dedicated function.

Request – USB3.0 writes 64B to EP0F:

Address

0000 55 00 01 00 00 00 00 00 00 DF 12 34 00 00 00 00

0010 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

0020 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

0030 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

Response – USB3.0 host reads 64B from EP8F:

Address

0000 55 01 01 00 00 00 00 00 00 00 00 00 00 00 00 00

0010 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

0020 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

0030 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

## Accessing LMS7002M registers

Configuration memory which is inside LMS7002M can be accessed using USB3.0 host via EP0F and EP8F endpoints. See **LMS64C\_protocol** document for protocol structure and description of commands used in examples. Registers map of LMS7002M can be found in [LMS7002M – Multi-Band, Multi-Standard MIMO, Programming and Calibration Guide](https://github.com/myriadrf/LMS7002M-docs/blob/master/LMS7002M_Programming_and_Calibration_Guide_v31r05.pdf).

**Read** – 64byte packet containing request command “CMD\_LMS7002\_RD” has to be sent to EP0F endpoint and 64 bytes response packet has to be read from EP8F endpoint. Read example reads 0x0020 address register value, which is 0xFFFF by default.

Request – USB3.0 writes 64B to EP0F:

Address

0000 22 00 01 00 00 00 00 00 00 20 00 00 00 00 00 00

0010 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

0020 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

0030 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

Response – USB3.0 host reads 64B from EP8F:

Address

0000 22 01 01 00 00 00 00 00 00 00 FF FF 00 00 00 00

0010 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

0020 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

0030 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

**Write** – 64byte packet containing request command “CMD\_LMS7002\_WR” has to be sent to EP0F endpoint and 64 bytes response packet has to be read from EP8F endpoint. Write example writes 0xE4E4 value to 0x0024 address.

Request – USB3.0 writes 64B to EP0F:

Address

0000 21 00 01 00 00 00 00 00 00 24 E4 E4 00 00 00 00

0010 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

0020 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

0030 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

Response – USB3.0 host reads 64B from EP8F:

Address

0000 21 01 01 00 00 00 00 00 00 00 00 00 00 00 00 00

0010 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

0020 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

0030 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

## Periphery control

**LED control -** modify FPGA register as showed in **Table 26** to turn on and change colour of FPGA\_LED2.

Table 26 FPGA\_LED2 control example

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **N** | **CMD** | **Address (HEX)** | **Value (HEX)** | **Description** |
| 1 | WR | 001A | 0010 | Override FPGA\_LED2 control |
| 2 | WR | 001A | 0030 | Turn on FPGA\_LED2\_R (red is on, green - off) |
| 3 | WR | 001A | 0050 | Turn on FPGA\_LED2\_G (green is on, red - off) |

## Configuring FPGA PLL module

To configure PLLs of pll\_top module LMS7002M chip has to be already configured and valid clock sources provided to LMS\_MCLK1 (connected to txpll\_top module) and LMS\_MCLK2 (connected to rxpll\_top module) pins. For LMS7002M chip configuration see chapter 4.2 Accessing LMS7002M registers.

Configuration of pll\_top module can be done by accessing FPGA registers see chapter **4.1 Accessing FPGA registers**. For register description see chapter **3.3 Softcore processor – nios\_cpu**.

PLL output frequency Fout can be calculated using following equation:

(1); (2); (3);

where *Fref*- PLL reference frequency, *FVCO* – VCO frequency, *FOUT* – Output frequency. See Cyclone IV datasheet for allowed frequency ranges.

### RX PLL module - rxpll\_top configuration (auto phase shift mode)

This example assumes that LMS7002M chip is already configured, outputs 20MHz clock on LMS\_MCLK2 pin and LMS\_DIQ2 interface outputs constant IQ values (I=0xAAA, Q=0x555). See **Table 27** for configuration sequence.

Table 27 rxpll\_top configuration sequence in auto phase shift mode

| **N** | **CMD** | **Address (HEX)** | **Value (HEX)** | **Description** |
| --- | --- | --- | --- | --- |
| 1 | WR | 0005 | 0000 | Turn off direct clocking |
| 2 | WR | 0025 | 01F0 | Set PLL parameters |
| 0023 | 0008 | Set PLL index to 1 and rest bits to zero |
| 3 | WR | 0023 | 0008 | Set PLL index to 1 and rest bits to zero |
| 0026 | 000A | N, M division bypass and odd division values. N, M division is not bypassed, odd division values enabled |
| 002A | 0201 | N, count value = 0x02 + 0x01 = 0x03 (3 DEC) |
| 002B | 6261 | M count value = 0x62 + 0x61 = 0xC3 (195 DEC) |
| 002E | 2120 | C0 count value = 0x21 + 0x20 = 0x41 (65 DEC) |
| 002F | 2120 | C1 count value = 0x21 + 0x20 = 0x41 (65 DEC) |
| 0027 | 555a | Counter C0-C7 bypass and odd division control bits. C0 and C1 not bypassed, others bypassed. C0 and C1 odd division values enabled, others not enabled. |
| 0028 | 5555 | Counter C7-C15 bypass and odd division control bits. All counters are bypassed. |
| 0023 | 0009 | Trigger reconfiguration for PLL index 1. |
| 4 | WR | 0023 | 6308 | Release PLL reconfiguration bit, set PLL index - 1, cnt index - 3, phase shift - up, phase shift mode - auto |
| 0024 | 0207 | Phase shift value = 0x0207 (519 DEC), represents 360 degrees (range in which auto phase shift is executed) |
| 0023 | 630a | Trigger auto phase shift for PLL index 1, cnt index 3, phase shift - up, phase shift mode - auto |
| 5 | RD | 0021 | - | Read PLL configuration status register and wait for configuration done (0x0005) |
| 6 | WR | 0023 | 6308 | Release PLL phase shift bit, set PLL index - 1, cnt index - 3, phase shift - up, phase shift mode - auto |

### TX PLL module - txpll\_top configuration (auto phase shift mode)

This example assumes that LMS7002M chip is already configured, outputs 20MHz clock on LMS\_MCLK1-2 pins, LimeLight digital loopback is enabled and FPGA rxpll\_top module is already configured. See **Table 28** for configuration sequence.

Table 28 txpll\_top configuration sequence in auto phase shift mode

| **N** | **CMD** | **Address (HEX)** | **Value (HEX)** | **Description** |
| --- | --- | --- | --- | --- |
| 1 | WR | 000A | 0200 | Enable TX test pattern |
| 2 | WR | 0005 | 0000 | Turn off direct clocking |
| 3 | WR | 0025 | 01F0 | Set PLL parameters |
| 0023 | 0000 | Set PLL index to 0 and rest bits to zero |
| 4 | WR | 0023 | 0000 | Set PLL index to 0 and rest bits to zero |
| 0026 | 000A | N, M division bypass and odd division values. N, M division is not bypassed, odd division values enabled |
| 0002A | 0201 | N, count value = 0x02 + 0x01 = 0x03 (3 DEC) |
| 002B | 6261 | M count value = 0x62 + 0x61 = 0xC3 (195 DEC) |
| 002E | 2120 | C0 count value = 0x21 + 0x20 = 0x41 (65 DEC) |
| 002F | 2120 | C1 count value = 0x21 + 0x20 = 0x41 (65 DEC) |
| 0027 | 555a | Counter C0-C7 bypass and odd division control bits. C0 and C1 not bypassed, others bypassed. C0 and C1 odd division values enabled, others not enabled. |
| 0028 | 5555 | Counter C7-C15 bypass and odd division control bits. All counters are bypassed. |
| 0023 | 0001 | Trigger reconfiguration for PLL index 0. |
| 5 | WR | 0023 | 6300 | Release PLL reconfiguration bit, set PLL index - 0, cnt index - 3, phase shift - up, phase shift mode - auto |
| 0024 | 0207 | Phase shift value = 0x0207 (519 DEC), represents 360 degrees (range in which auto phase shift is executed) |
| 0023 | 6302 | Trigger auto phase shift for PLL index 0, cnt index 3, phase shift - up, phase shift mode - auto |
| 6 | RD | 0021 | - | Read PLL configuration status register and wait for configuration done (0x0005) |
| 7 | WR | 0023 | 6300 | Release PLL phase shift bit, set PLL index - 0, cnt index - 3, phase shift - up, phase shift mode - auto |

## Controlling TX and RX data stream

Data stream can be enabled when LMS7002M chip and FPGA PLL modules are configured. See chapters **4.2 Accessing LMS7002M registers** and **4.4 Configuring FPGA PLL module.**

**To enable TX and RX data stream –** follow FPGA register write sequence described in **Table 29**.

Table 29 enabling TX and RX data stream

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **N** | **CMD** | **Address (HEX)** | **Value (HEX)** | **Description** |
| 1 | WR | 000A | 0000 | Stop data stream |
| 2 | WR | 0009 | 0000 | Clear packet loss and reset timestamp bits. |
| 3 | WR | 0009 | 0003 | Clear packet loss flag and reset timestamp. |
| 4 | WR | 0009 | 0000 | Clear packet loss and reset timestamp bits. |
| 5 |  |  |  | Reset USB3.0 EP01 end EP81 endpoints (Use CMD\_STREAM\_RST command) |
| 6 | WR | 0008 | 102 | Set sample width -12, mode - TRXIQ, DDR - enabled, TRXIQ\_PULSE mode - disabled, packet synchronization - enabled |
| 7 | WR | 0007 | 0001 | Set active channels - 1 |
| 8 | WR | 000A | 0001 | Start stream |

**To disable** **TX and RX data stream –** follow FPGA register write sequence described in **Table 30.**

Table 30 disabling TX and RX data stream

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **N** | **CMD** | **Address (HEX)** | **Value (HEX)** | **Description** |
| 1 | WR | 000A | 0000 | Stop data stream |

## Using WFM player

WFM player requires that onboard clock generator Si5351C has to be configured to output 27MHz clock on CLK0 output and LMS7002M has to be configured. See **Table 31** for data loading sequence.

Table 31 WFM data loading

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **N** | **CMD** | **Address (HEX)** | **Value (HEX)** | **Description** |
| 1 | WR | 000C | 0003 | Enable both channels |
| 2 | WR | 000E | 0002 | Set sample width to 16bit mode |
| 4 | WR | 000D | 0006 | Enable WFM loading |
| 5 |  |  |  | Load WFM data to EP01 endpoint |
| 6 | WR | 000D | 0002 | Disable WFM loading, start playing file |